Lever sets for standard doors
Lever version L56 Berlin
by KARCHER DESIGN

Lever handle on plate 224 x 44 mm,
with dual fixing and nylon floating bearing,
sprung loaded inner plate with attached lever,
timber screws, visible fixed,
8mm offset drilled spindle,
standard door thickness: 37 - 43 mm
diameter of handle: 22 x 9 mm,

Options:
UN - latch
BB 57 or 72 mm - supplied with lever key
PZ 48, 72 or 92 mm - supplied with euro profile
BAD 57 or 78 mm - supplied with bathroom turn/release set
 
Plate: satin polished brass (finish code 20)
Handle: satin polished brass
Karcher article no.:
L56 UN 20 - latch
L56 BB0 20 - supplied with lever key
L56 PZ0 20 - supplied with euro profile
L56 BAD 20 - supplied with bathroom turn/release set

Dimensional detail:

44 mm

144

80

 60

 133

22/9

69

133