Lever sets for standard doors
Lever version RL37 Verona
by KARCHER DESIGN

Lever handle on plate 242 x 46,5 mm,
with dual fixing and nylon floating bearing,
sprung loaded inner plate with attached lever,
M4 bolt through fixing,
8mm offset drilled spindle,
standard door thickness: 37 - 43 mm
diameter of handle: 24x17 mm, oval,

Options:
UN - latch
BB 57 or 72 mm - supplied with lever key
PZ 48, 72 or 92 mm - supplied with euro profile
BAD 57 or 78 mm - supplied with bathroom turn/release set

Plate: satin nickel (finish code 60)
Handle: satin stainless steel
Karcher article no.:
RL37 UN 60 - latch
RL37 BB0 60 - supplied with lever key
RL37 PZ0 60 - supplied with euro profile
RL37 BAD 60 - supplied with bathroom turn/release set

46,5 mm

150

90

135

75

130

56

24

17

Dimensional detail: